**POWER SUPPLY**

**Features**

• N-channel

• Depletion mode

• dv /dt rated

• Available with V GS(th) indicator on reel

• Pb-free lead-plating; RoHS compliant

• Halogen-free according to AEC61249-2-21

• Qualified according to AEC Q101

Boom list and gerber file are given in the description.